#!/bin/bash

PIN_PAPOWER=5

# init
gpio mode $PIN_PAPOWER output

# command
if [[ "$1" == "on" ]]; then
	gpio write $PIN_PAPOWER 1
elif [[ "$1" == "off" ]]; then
	gpio write $PIN_PAPOWER 0
elif [[ "$1" == "read" ]]; then
	gpio read $PIN_PAPOWER
else
	gpio toggle $PIN_PAPOWER
fi
	
